[bookmark: _opx9bwsq832i]What is the INSTA Heat Press?
· A giant iron!
· Like our current heat press, this is a large heated metal plate.
· Used for:
· Direct to Film, Dye Sublimation, Heat Transfer Vinyl, White Toner Ink, Fabric Interfacing 
[bookmark: _2evm4l2x24uv]What can you make with it?
· Items Benefit DMS’s Function and Appearance
· Signage and Promotional Items for DMS
· Coffin Race Shirts
· Subiefest Shirts
· Tour Day Sign
· Tabletop Sig Play Mats
· To press items bigger than 16x20!
· Arcade Cabinets
· Cosplay bodysuits
· Photographs/Art Canvas Prints
· Fabric
· Clothing
· Metal & Wood Signs
[bookmark: _kbpgbqmcuto3]Why is it good for DMS?
· Exclusivity/ Excitement/Draw
· Heat presses are difficult to find at this size.
· Graphic Designers are excited to have access to a larger tool.
· Already getting more graphics volunteers due to heat press interest.
· Iteration
· Makers can easily test materials samples and layouts, this is not cost-effective with a sign shop or fabric shop such as Spoonflower.
· DMS Needs It!
· Will help us quickly redecorate DMS after/during construction
· DMS branding, such as Apparel, Decor, Signage.
[bookmark: _l1cgtyk1t2zf]How did it get to DMS?
· Donor purchased heat press for testing, and offered it to DMS once testing was complete.
· Donor also wishes to tour DMS during the month of October
· James emailed donor at the time of donation receipt
· Donor stated they may also wish to buy a block of memberships for their employees
[bookmark: _9t3aoaf7uej2]How Hot is It?
· Heats to 3-400Degrees F, presses materials flat.
· Efficient, heat is well contained within the unit.
· Heat cannot be felt at all outside of Vector
[image: ]
[bookmark: _c22mb6g2r6zf]What are the needs of the Heat Press?
· 3 Phase, 208 power- as close to the breaker box as possible. (per Jeff)
· Dust Free Environment- dust and dirt from workshops will ruin prints.
· 20in of space around it.
· Air Pressure
· Extant- an air hose may be connected from the Machine Shop
· Ideal- air pressure drop from line in Jewelry
· Glass Kilns already need an extension of the Jewelry line
· Most piping is already in DMS storage
· Cost minimal
· Heat Venting- Optional
· Optional because heat is not excessive.
· To maximize cooling efficiency, a heat chimney could be easily added to the Glass Kiln Venting.
· All venting/ flue parts already gathered.
[bookmark: _5fmxyx33d6fu]Why is the INSTA in Vector?
· Vector can use it in arcade cabinets, play decks, and signage for our area
· It allows Vector to benefit DMS
· The location is logical- near other types of Printmaking
· Vector meets the power and cleanliness requirements of the machine.
[bookmark: _7n704ebf5qj]FAQ: 
[bookmark: _939m27xyqfu7]Does Vector plan more printer purchases?
· Direct to Film No, Never.
·  We already turned down a free Direct To Film Printer from this donor.
Requires fume extraction, is the size of a car, must be kept at 75f, maintenance every 24-48hrs.
· UV Printer: No, Never.
	Similar to above, high maintenance, fumes, maintenance.
· Direct to Garment No Purchase, will analyze if offered one for free.
· Not likely, limited to specific use cases.
· Analysis Requirements:
· Low scheduled maintenance cycles, Cost, Maintenance Schedules & costs, Fumes, Use Cases
· Large Format Dye Sublimation Printer.
· Possible ask, but not in 2024, not likely in 2025.
· only after deliberation, growth, and cost-benefit analysis.
· Considerations before an ask:
· Low maintenance 
· Low Cost. (Currently 5-7k for a new machine)
· Costs have fallen significantly, if they fall further it may be a reasonable buy or accepted donation in the coming years. 
· Fumes: None
· Use Cases: Broad.
[bookmark: _ies6qe53x4ku]How will Vector Prevent Abuse/Misuse of the Press?
· Intended use will be taught in class.
· If a user’s business model is dependent upon DMS tools, this is beyond intended use.
· Speed is set slow, and is slow enough not to be profitable for a business
· Speed control is difficult to find, and will be covered with a lockbox.
· Tampering w/ the lockbox will result in immediate and permanent tool ban
· Each press must be triggered manually.
· Auto button will be covered with lockbox
· Tampering with lockbox will result in immediate & permanent ban.
· Ideal:  RFID interlock will be added to press control box as a cover, and a log of use will be pulled monthly, user numbers that come up frequently will be queried/ video pulled.
· Currently: Manual logging
· Date/Name/Starting number of presses/ending # of presses (on the control unit)
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